Torque Specs
These specs may not be correct for your application.
Verify your engine specs with a service manual for your year and model. 
always torque bolts in three equal increments
Bolts or Parts	Lube or Sealer	Torque to:	
Main Caps	Engine Oil	105 ft-lbs.	
Warning!!! 
If you are using ARP bolts, you MUST use
their specs. Click Here!			
Connecting Rod Bolts 351C
*Boss 351C	Engine Oil	45 ft-lbs.
*50 ft-lbs.	
Cylinder Heads 351C
*Boss 351C	Engine oil 
(blind hole)
Sealer
(water jacket)	105 ft-lbs.
*125 ft-lbs.	
Rocker Arms	Engine Oil	20 ft-lbs.	
Oil Pump	Engine Oil	25 ft-lbs.	
Oil Pan	Engine Oil	12 ft-lbs.	
Camshaft Thrust Plate	Thread Locker	12 ft-lbs.	
Cam Bolt (upper gear)	Thread Locker	40 ft-lbs.	
Front Cover	Engine Oil	20 ft-lbs.	
Intake Manifold 5/16 Bolts
(Cast Iron Heads) *3/8 Bolts	Non- Hardening Sealer	25 ft-lbs.
*30 ft-lbs.	
Valve Cover	Engine Oil	10 ft-lbs.	
Flexplate (Automatic)
Flywheel (Clutch) 	Thread Locker	85 ft-lbs.	
Clutch Pressure Plate	Thread Locker	35 ft-lbs.	
Centerbolt
(Harmonic Damper)	Thread Locker	90 ft-lbs.	
Bellhousing
(Transmission to Block)